
Zener DC-to-DC Converter


## Procedure

Some devices (for example, the ultrasonic sensor in your kit) are designed to work with a maximum voltage supply below the 9-volts that you have in your kit. This exercise will allow you to complete a design for a 9-volt-to-5-volt dc converter. The end result will be something that behaves much like a 5-volt battery although with a higher effective resistance than the original battery.





***Figure 1:*** *A 9VDC-to-5VDC Zener-regulator circuit (top schematic).*

The Zener diode (<https://en.wikipedia.org/wiki/Zener_diode>) is a special diode that allows current to flow in ***either*** direction once a turn-on voltage has been reached in that polarity. While the forward-bias turn-on voltage is typical of the semiconductor material, the reverse-bias turn-on voltage (also called a “breakdown” voltage although it does not imply damage) can be designed to take on different turn-on voltage for different projects. The IV characteristic of a Zener diode is demonstrated in Figure 2.



***Figure 2:*** *Current-voltage characteristic of a Zener diode with a breakdown voltage labeled “”.*


The special diode in your kit (it will be separate with thicker wires than the “signal” diodes that you may have already used) is a Zener diode with a reverse-bias turn-on voltage near 5 volts. ***For our analysis purposes***, you can imagine the Zener diode in Figure 1 to be a regular diode oriented in the downward direction with a (sharp) turn-on voltage of .




***Figure 3:*** *Select details from the Zener datasheet to aid with orientation in your circuit.*

Before you build, as a design engineer, you will need to perform some analysis to verify both safety and function. Consider these facts and answer the following questions.

1. We want to use this new 5-volt supply to operate both the ultrasonic (US) sensor which draws about 15 mA as well as a Schmitt-trigger oscillator which draws up to 35 mA. Using Kirchhoff’s Voltage Law on the loop below, what is a good value to represent the resistive load, , to represent both the current draw of the oscillator and the current draw of the US sensor? Explain.



1. You know that a charged capacitor draws no current. Determine the range of values appropriate for to provide to the load. **Hint**: You need to use Kirchhoff’s Current Law to find the range of that guarantees while the Zener diode operates at the breakdown voltage, . Show your work.



1. Now, we must consider an engineering tradeoff. Choosing small will provide a 5-volt source with a smaller effective resistance and, therefore, capable of providing more current to the load if using this for other applications. However, a small will also mean *more power dissipated* by even when the load is drawing little current or disconnected entirely! Consider the resistor values in your kit and design a resistive network for that meets these goals:

* The effective resistance of your network, , is *near* the largest value in the range, but does not exceed the range so that may be drawn by the load.
* Each resistor used in the resistive network for dissipates less than (our resistors are rated for , so we are being a little conservative here).
* The resistors come from the limited values available in your kit, the contents of which may be found at <https://ece.illinois.edu/academics/ugrad/lab-kits/ece110>.

Explain your reasoning as you show your work.

1. Sketch the schematic of Figure 1 explicitly showing your resistor network for .
2. How would you redesign your resistive network if you needed it to be capable of delivering more current, say , to the load? Explain.

**You may now build the circuit according to your design.**

1. Use your 9-volt battery and the M2k’s voltmeter or oscilloscope to validate your design. Submit a video demonstrating the 9-volt input and 5-volt output with two different resistive loads, .

## Learning Objectives

* Ability to map a circuit design onto the breadboard in a functional and clean manner.
* Demonstrate the ability to use the M2k to monitor voltage.
* Design by considering both safety and function of a device.
* Ability to troubleshoot problems that occur during a build.